set PREVIEW_MODE "Key Dumper\n \nWorking..."

# Boot9

set BOOT9_BIN "M:/boot9.bin"

fget $[BOOT9_BIN]@D9D0:10 KEYX_2C
set KEYX_2D $[KEYX_2C]
set KEYX_2E $[KEYX_2C]
set KEYX_2F $[KEYX_2C]
fget $[BOOT9_BIN]@D9E0:10 KEYX_30
set KEYX_31 $[KEYX_30]
set KEYX_32 $[KEYX_30]
set KEYX_33 $[KEYX_30]
fget $[BOOT9_BIN]@D9F0:10 KEYX_34
set KEYX_35 $[KEYX_34]
set KEYX_36 $[KEYX_34]
set KEYX_37 $[KEYX_34]
fget $[BOOT9_BIN]@DA00:10 KEYX_38
set KEYX_39 $[KEYX_38]
set KEYX_3A $[KEYX_38]
set KEYX_3B $[KEYX_38]
fget $[BOOT9_BIN]@DA10:10 KEYX_3C
fget $[BOOT9_BIN]@DA20:10 KEYX_3D
fget $[BOOT9_BIN]@DA30:10 KEYX_3E
fget $[BOOT9_BIN]@DA40:10 KEYX_3F

fget $[BOOT9_BIN]@DA50:10 KEYY_04
fget $[BOOT9_BIN]@DA60:10 KEYY_05
fget $[BOOT9_BIN]@DA70:10 KEYY_06
fget $[BOOT9_BIN]@DA80:10 KEYY_07
fget $[BOOT9_BIN]@DA90:10 KEYY_08
fget $[BOOT9_BIN]@DAA0:10 KEYY_09
fget $[BOOT9_BIN]@DAB0:10 KEYY_0A
fget $[BOOT9_BIN]@DAC0:10 KEYY_0B

fget $[BOOT9_BIN]@DAD0:10 KEYN_0D
fget $[BOOT9_BIN]@DBA0:10 KEYN_2D
fget $[BOOT9_BIN]@DBB0:10 KEYN_32
fget $[BOOT9_BIN]@DBC0:10 KEYN_36
fget $[BOOT9_BIN]@DBD0:10 KEYN_38

# NATIVE_FIRM

if chk $[ONTYPE] "N3DS"
    if not find 1:/title/00040138/20000002/content/????????.app NATIVE_FIRM_APP
        echo "New 3DS NATIVE_FIRM not found."
        goto Exit
    end
    set EXPECTED_NATIVE_FIRM_VER "1F00"
    set KEYY_2E_OFFSET "66504"
    set KEYY_39_NFC_OFFSET "66524"
    set COMMON_0_OFFSET "6CE51"
    set COMMON_1_OFFSET "6CE65"
    set COMMON_2_OFFSET "6CE79"
    set COMMON_3_OFFSET "6CE8D"
    set COMMON_4_OFFSET "6CEA1"
    set COMMON_5_OFFSET "6CEB5"
else
    if not find 1:/title/00040138/00000002/content/????????.app NATIVE_FIRM_APP
        echo "Old 3DS NATIVE_FIRM not found."
        goto Exit
    end
    set EXPECTED_NATIVE_FIRM_VER "1F00"
    set KEYY_2E_OFFSET "66488"
    set KEYY_39_NFC_OFFSET "664A8"
    set COMMON_0_OFFSET "6CDC1"
    set COMMON_1_OFFSET "6CDD5"
    set COMMON_2_OFFSET "6CDE9"
    set COMMON_3_OFFSET "6CDFD"
    set COMMON_4_OFFSET "6CE11"
    set COMMON_5_OFFSET "6CE25"
end
set NATIVE_FIRM_EXTHEADER "G:/extheader.bin"
set NATIVE_FIRM_ENCRYPTED "G:/exefs/.firm"
set NATIVE_FIRM_DECRYPTED "$[GM9OUT]/native.firm"
set PROCESS9_CODE "G:/0004013000003000.Process9/exefs/.code"

imgmount $[NATIVE_FIRM_APP]

fget $[NATIVE_FIRM_EXTHEADER]@E:2 NATIVE_FIRM_VER
if not chk $[NATIVE_FIRM_VER] $[EXPECTED_NATIVE_FIRM_VER]
    echo "Unsupported NATIVE_FIRM version.\nThis script requires the latest 3DS firmware.\n\nExpected $[EXPECTED_NATIVE_FIRM_VER], got $[NATIVE_FIRM_VER]"
    goto Exit
end

cp -w $[NATIVE_FIRM_ENCRYPTED] $[NATIVE_FIRM_DECRYPTED]
decrypt $[NATIVE_FIRM_DECRYPTED]

imgumount

imgmount $[NATIVE_FIRM_DECRYPTED]

fget $[PROCESS9_CODE]@$[KEYY_2E_OFFSET]:10 KEYY_2E
set KEYY_31 $[KEYY_2E]
set KEYY_39_DLP $[KEYY_2E]
fget $[PROCESS9_CODE]@$[KEYY_39_NFC_OFFSET]:10 KEYY_39_NFC
fget $[PROCESS9_CODE]@$[COMMON_0_OFFSET]:10 COMMON_0
fget $[PROCESS9_CODE]@$[COMMON_1_OFFSET]:10 COMMON_1
fget $[PROCESS9_CODE]@$[COMMON_2_OFFSET]:10 COMMON_2
fget $[PROCESS9_CODE]@$[COMMON_3_OFFSET]:10 COMMON_3
fget $[PROCESS9_CODE]@$[COMMON_4_OFFSET]:10 COMMON_4
fget $[PROCESS9_CODE]@$[COMMON_5_OFFSET]:10 COMMON_5

imgumount
rm -o -s $[NATIVE_FIRM_DECRYPTED]

# NFC

if chk $[ONTYPE] "N3DS"
    if not find 1:/title/00040130/20004002/content/????????.app NFC_APP
        echo "New 3DS NFC not found."
        goto Exit
    end
    set EXPECTED_NFC_VER "0700"
    set NFC_PHRASE_0_OFFSET "355EE"
    set NFC_SEED_0_OFFSET "355FC"
    set NFC_HMAC_KEY_0_OFFSET "3560A"
    set NFC_PHRASE_1_OFFSET "3561A"
    set NFC_SEED_1_OFFSET "35628"
    set NFC_HMAC_KEY_1_OFFSET "35638"
    set NFC_IV_OFFSET "35648"
else
    if not find 1:/title/00040130/00004002/content/????????.app NFC_APP
        echo "Old 3DS NFC not found."
        goto Exit
    end
    set EXPECTED_NFC_VER "0800"
    set NFC_PHRASE_0_OFFSET "17382"
    set NFC_SEED_0_OFFSET "17390"
    set NFC_HMAC_KEY_0_OFFSET "1739E"
    set NFC_PHRASE_1_OFFSET "173AE"
    set NFC_SEED_1_OFFSET "173BC"
    set NFC_HMAC_KEY_1_OFFSET "173CC"
    set NFC_IV_OFFSET "173DC"
end
set NFC_EXTHEADER "G:/extheader.bin"
set NFC_CODE "$[GM9OUT]/nfc_code.bin"

imgmount $[NFC_APP]

fget $[NFC_EXTHEADER]@E:2 NFC_VER
if not chk $[NFC_VER] $[EXPECTED_NFC_VER]
    echo "Unsupported NFC module version.\nThis script requires the latest 3DS firmware.\n\nExpected $[EXPECTED_NFC_VER], got $[NFC_VER]"
    goto Exit
end

imgumount

extrcode $[NFC_APP] $[NFC_CODE]

fget $[NFC_CODE]@$[NFC_PHRASE_0_OFFSET]:E NFC_PHRASE_0
fget $[NFC_CODE]@$[NFC_SEED_0_OFFSET]:E NFC_SEED_0
fget $[NFC_CODE]@$[NFC_HMAC_KEY_0_OFFSET]:10 NFC_HMAC_KEY_0

fget $[NFC_CODE]@$[NFC_PHRASE_1_OFFSET]:E NFC_PHRASE_1
fget $[NFC_CODE]@$[NFC_SEED_1_OFFSET]:10 NFC_SEED_1
fget $[NFC_CODE]@$[NFC_HMAC_KEY_1_OFFSET]:10 NFC_HMAC_KEY_1

fget $[NFC_CODE]@$[NFC_IV_OFFSET]:10 NFC_IV

rm -o -s $[NFC_CODE]

# GodMode9 Key Database

set KEY_DB "V:/aeskeydb.bin"
set KEY_DB_18X "K:/slot0x18KeyX.ret.bin"
set KEY_DB_19X "K:/slot0x19KeyX.ret.bin"
set KEY_DB_1AX "K:/slot0x1AKeyX.ret.bin"
set KEY_DB_1BX "K:/slot0x1BKeyX.ret.bin"
set KEY_DB_1CX "K:/slot0x1CKeyX.ret.bin"
set KEY_DB_1DX "K:/slot0x1DKeyX.ret.bin"
set KEY_DB_1EX "K:/slot0x1EKeyX.ret.bin"
set KEY_DB_1FX "K:/slot0x1FKeyX.ret.bin"
set KEY_DB_25X "K:/slot0x25KeyX.ret.bin"
set KEY_DB_24Y "K:/slot0x24KeyY.bin"
set KEY_DB_2FY "K:/slot0x2FKeyY.ret.bin"

imgmount $[KEY_DB]

fget $[KEY_DB_18X]@0:10 KEYX_18
fget $[KEY_DB_19X]@0:10 KEYX_19
fget $[KEY_DB_1AX]@0:10 KEYX_1A
fget $[KEY_DB_1BX]@0:10 KEYX_1B
fget $[KEY_DB_1CX]@0:10 KEYX_1C
fget $[KEY_DB_1DX]@0:10 KEYX_1D
fget $[KEY_DB_1EX]@0:10 KEYX_1E
fget $[KEY_DB_1FX]@0:10 KEYX_1F
fget $[KEY_DB_25X]@0:10 KEYX_25

fget $[KEY_DB_24Y]@0:10 KEYY_24
fget $[KEY_DB_2FY]@0:10 KEYY_2F

imgumount

# Write Keys To File

set OUT "0:/gm9/aes_keys.txt"

dumptxt $[OUT] "# KeyX"
dumptxt -p $[OUT] ""

dumptxt -p $[OUT] "slot0x18KeyX=$[KEYX_18]"
dumptxt -p $[OUT] "slot0x19KeyX=$[KEYX_19]"
dumptxt -p $[OUT] "slot0x1AKeyX=$[KEYX_1A]"
dumptxt -p $[OUT] "slot0x1BKeyX=$[KEYX_1B]"
dumptxt -p $[OUT] "slot0x1CKeyX=$[KEYX_1C]"
dumptxt -p $[OUT] "slot0x1DKeyX=$[KEYX_1D]"
dumptxt -p $[OUT] "slot0x1EKeyX=$[KEYX_1E]"
dumptxt -p $[OUT] "slot0x1FKeyX=$[KEYX_1F]"
dumptxt -p $[OUT] "slot0x25KeyX=$[KEYX_25]"
dumptxt -p $[OUT] "slot0x2CKeyX=$[KEYX_2C]"
dumptxt -p $[OUT] "slot0x2DKeyX=$[KEYX_2D]"
dumptxt -p $[OUT] "slot0x2EKeyX=$[KEYX_2E]"
dumptxt -p $[OUT] "slot0x2FKeyX=$[KEYX_2F]"
dumptxt -p $[OUT] "slot0x30KeyX=$[KEYX_30]"
dumptxt -p $[OUT] "slot0x31KeyX=$[KEYX_31]"
dumptxt -p $[OUT] "slot0x32KeyX=$[KEYX_32]"
dumptxt -p $[OUT] "slot0x33KeyX=$[KEYX_33]"
dumptxt -p $[OUT] "slot0x34KeyX=$[KEYX_34]"
dumptxt -p $[OUT] "slot0x35KeyX=$[KEYX_35]"
dumptxt -p $[OUT] "slot0x36KeyX=$[KEYX_36]"
dumptxt -p $[OUT] "slot0x37KeyX=$[KEYX_37]"
dumptxt -p $[OUT] "slot0x38KeyX=$[KEYX_38]"
dumptxt -p $[OUT] "slot0x39KeyX=$[KEYX_39]"
dumptxt -p $[OUT] "slot0x3AKeyX=$[KEYX_3A]"
dumptxt -p $[OUT] "slot0x3BKeyX=$[KEYX_3B]"
dumptxt -p $[OUT] "slot0x3CKeyX=$[KEYX_3C]"
dumptxt -p $[OUT] "slot0x3DKeyX=$[KEYX_3D]"
dumptxt -p $[OUT] "slot0x3EKeyX=$[KEYX_3E]"
dumptxt -p $[OUT] "slot0x3FKeyX=$[KEYX_3F]"

dumptxt -p $[OUT] ""
dumptxt -p $[OUT] "# KeyY"
dumptxt -p $[OUT] ""

dumptxt -p $[OUT] "slot0x04KeyY=$[KEYY_04]"
dumptxt -p $[OUT] "slot0x05KeyY=$[KEYY_05]"
dumptxt -p $[OUT] "slot0x06KeyY=$[KEYY_06]"
dumptxt -p $[OUT] "slot0x07KeyY=$[KEYY_07]"
dumptxt -p $[OUT] "slot0x08KeyY=$[KEYY_08]"
dumptxt -p $[OUT] "slot0x09KeyY=$[KEYY_09]"
dumptxt -p $[OUT] "slot0x0AKeyY=$[KEYY_0A]"
dumptxt -p $[OUT] "slot0x0BKeyY=$[KEYY_0B]"
dumptxt -p $[OUT] "slot0x24KeyY=$[KEYY_24]"
dumptxt -p $[OUT] "slot0x2EKeyY=$[KEYY_2E]"
dumptxt -p $[OUT] "slot0x2FKeyY=$[KEYY_2F]"
dumptxt -p $[OUT] "slot0x31KeyY=$[KEYY_31]"

dumptxt -p $[OUT] ""
dumptxt -p $[OUT] "# DLP/NFC KeyY (slot 0x39)"
dumptxt -p $[OUT] ""

dumptxt -p $[OUT] "dlpKeyY=$[KEYY_39_DLP]"
dumptxt -p $[OUT] "nfcKeyY=$[KEYY_39_NFC]"

dumptxt -p $[OUT] ""
dumptxt -p $[OUT] "# Ticket Common KeyY (slot 0x3D)"
dumptxt -p $[OUT] ""

dumptxt -p $[OUT] "common0=$[COMMON_0]"
dumptxt -p $[OUT] "common1=$[COMMON_1]"
dumptxt -p $[OUT] "common2=$[COMMON_2]"
dumptxt -p $[OUT] "common3=$[COMMON_3]"
dumptxt -p $[OUT] "common4=$[COMMON_4]"
dumptxt -p $[OUT] "common5=$[COMMON_5]"

dumptxt -p $[OUT] ""
dumptxt -p $[OUT] "# KeyN"
dumptxt -p $[OUT] ""

dumptxt -p $[OUT] "slot0x0DKeyN=$[KEYN_0D]"
dumptxt -p $[OUT] "slot0x2DKeyN=$[KEYN_2D]"
dumptxt -p $[OUT] "slot0x32KeyN=$[KEYN_32]"
dumptxt -p $[OUT] "slot0x36KeyN=$[KEYN_36]"
dumptxt -p $[OUT] "slot0x38KeyN=$[KEYN_38]"

dumptxt -p $[OUT] ""
dumptxt -p $[OUT] "# NFC Secrets"
dumptxt -p $[OUT] ""

dumptxt -p $[OUT] "nfcSecret0Phrase=$[NFC_PHRASE_0]"
dumptxt -p $[OUT] "nfcSecret0Seed=$[NFC_SEED_0]"
dumptxt -p $[OUT] "nfcSecret0HmacKey=$[NFC_HMAC_KEY_0]"
dumptxt -p $[OUT] "nfcSecret1Phrase=$[NFC_PHRASE_1]"
dumptxt -p $[OUT] "nfcSecret1Seed=$[NFC_SEED_1]"
dumptxt -p $[OUT] "nfcSecret1HmacKey=$[NFC_HMAC_KEY_1]"
dumptxt -p $[OUT] "nfcIv=$[NFC_IV]"

@Exit

